ORG **0000h**

**//AND OPERATION**

MOV A,#32h

ANL A,#45h

**//OR OPERATION**

MOV A,#0F2h

ORL A,#38h

**//NOT OPERATION**

MOV A,#31h

CPL A

CPL ACC.2

CPL PSW.3

**//XOR OPERATION**

MOV A,#22h

XRL A,#45h

**//CLEAR BIT(CLR)**

MOV A,#0FFh

CLR ACC.3

CLR A

**//SET BIT(SETB)**

MOV A,#00h

SETB ACC.0

END